**CORRIGENDUM**

**CONTRACT NOTICE**

**II.1.1) Contract Notice Title: Supply of firefighting truck for the needs of the Municipality of Botevgrad**  
**II.1.1) Contract Notice Reference Number:** **CB007.2.32.165 – PP2 – Supply 1A**

**VII. 1.1) Reason for change**

Modification of original information submitted by the contracting authority.

**VII.1.2) Text to be corrected in the original notice**

Section No **II.1.5) Estimated total value**

Instead of: ***Within the contract a supply, delivery, unloading, training of employees of the Contracting authority and services under the warranty period for Firefighting truck******- 1 pc (*** *Payload: ≤ 7500 kg, Movement: 4x4, Engine: Diesel, common rail or similar/or equivalent, Min. EURO 6, Min. 130 kW, Min. 2500 sm3, Seats: 2+1, locking of the rear differential and transfer box, Capacity of the water tank: Minimum 2000 1, Fire superstructure with dismount-capacity: Locking mechanism, with interchangeable parts, easily mount-dismount towards the chassis of the truck, Side sections (one by each side) for firefighting equipment: 2 pcs, Adjustable supports for provision parking of the superstructure after the dismount: 4 pcs, Type-membrane: min 40 bar pressure mill. 50 1/minute flow rate, Gasoline or diesel power generator: min.9 h.p. with an electrical starter; Reel with installed hose-pipe: min. 50 m, at the rear of the truck; Nozzle with spray-module, STORZ quick connection coupling, Training of the employers of the Contracting Authority)* ***is needed.***

Read: **Within the contract a supply, delivery, unloading, training of employees of the Contracting authority and services under the warranty period for Firefighting Truck – 1 pc. (Payload: ≤ 7500 kg, Movement: at least 4x2, Engine: Diesel, common rail or similar/or equivalent, Min. EURO 6, Min. 115 kW, Min. 2500 cm3, Seats: 2+1, Capacity of the water tank: Min. 2000 1, Fire superstructure with dismount-capacity: easily mount- dismount towards the chassis of the truck, Side sections (one by each side) for firefighting equipment: 2 pcs, Adjustable supports for provision parking of the superstructure after the dismount: 4 pcs, Pump: Type-membrane: min 40 bar pressure min. 50 1/minute flow rate, Gasoline or diesel power generator: min. 9 h.p. with an electrical starter; Reel with installed hose-pipe: min. 50 m, at the rear of the truck; Nozzle with spray-module: Included, STORZ quick connection coupling, Training of the employers of the Contracting Authority) is needed.**

Section No **IV.2.2) Time limit for submission of tenders or requests to participate**

Instead of: *Date: 09.09.2022*

Read: **Date: 16.09.2022**

Section No **IV.2.7) Conditions for opening of tenders**

Instead of: *Date: 12.09.2022*

Read: **Date: 19.09.2022**

**VII.2) Other additional information:**

**TEXT TO BE CORRECTED IN ADDITIONAL INFORMATION ABOUT THE CONTRACT NOTICE**

Section No **10.2. Selection criteria**

Instead of: 2) Technical capacity (based on items 5 and 6 of the request to participate form for service contracts and on items 5 and 6 of the tender form for supply contracts). The reference period which will be taken into account will be the last three years from submission deadline.

b. The candidate has provided supplies under at least 1 contract with a budget of at least 200 000 BGN in the field of supply of firefighting trucks and/or equivalent specialized vehicles and/or equivalent specialized equipment which was implemented at any moment during the reference period: *09.09.2019–09.09.2022.*

Read: 2) Technical capacity (based on items 5 and 6 of the request to participate form for service contracts and on items 5 and 6 of the tender form for supply contracts). The reference period which will be taken into account will be the last three years from submission deadline.

b. The candidate has provided supplies under at least 1 contract with a budget of at least 200 000 BGN in the field of supply of firefighting trucks and/or equivalent specialized vehicles and/or equivalent specialized equipment which was implemented at any moment during the reference period: **16.09.2019–16.09.2022.**

**TEXT TO BE CORRECTED IN INSTRUCTIONS TO TENDERERS**

Section No **2 Timetable**

Instead of:

|  |  |  |
| --- | --- | --- |
|  | **DATE** | **TIME** |
| **Clarification meeting / site visit (if any)** | Not applicable | Not applicable |
| **Deadline for requesting clarifications from the contracting authority** | *19.08.2022* | 17:30 |
| **Last date on which clarifications are issued by the contracting authority** | *01.09.2022* | - |
| **Deadline for submission of tenders** | As indicated in the Contract notice | 17:30 o’clock |
| **Tender opening session** | As indicated in the Contract Notice (IV.2.7) | 10:00 o’clock |
| **Notification of award to the successful tenderer** | *12.09.2022\** | - |
| **Signature of the contract** | *13.09.2022\** | - |

Read:

|  |  |  |
| --- | --- | --- |
|  | **DATE** | **TIME** |
| **Clarification meeting / site visit (if any)** | Not applicable | Not applicable |
| **Deadline for requesting clarifications from the contracting authority** | **26.08.2022** | 17:30 |
| **Last date on which clarifications are issued by the contracting authority** | **08.09.2022** | - |
| **Deadline for submission of tenders** | As indicated in the Contract notice | 17:30 o’clock |
| **Tender opening session** | As indicated in the Contract Notice (IV.2.7) | 10:00 o’clock |
| **Notification of award to the successful tenderer** | **19.09.2022\*** | - |
| **Signature of the contract** | **20.09.2022\*** | - |

**TEXT TO BE CORRECTED IN ANNEX II + III: TECHNICAL SPECIFICATIONS + TECHNICAL OFFER:**

Instead of: ***Firefighting Truck – 1 pc.***

*1 Payload: ≤ 7500 kg*

*2 Movement: 4x4*

*3 Engine: Diesel, common rail or similar/or equivalent   
Min. EURO 6  
Min. 130 kW  
Min. 2500 sm3*

*4 Gear box: manual, at least 6+1 gears*

*4.1. Transfer box: Fast and slow gears*

*5 Cabin  
Seats: 2+1  
Air conditioning: Manual  
Driver’s seat: 3-degree adjustable*

*6 Chassis and suspension:   
locking of the rear differential and transfer box: yes  
Semi-elliptical" leaf springs: yes  
Rear turn signal: yes  
Protection of the crankcase of engine: yes*

*7 Tires: Double rear tires R16, steel wheels 16"*

*8 Water tank:   
Capacity of the water tank: Minimum 2000 1*

*9 Special equipment:   
9.1 Fire superstructure with dismount-capacity: Locking mechanism, with interchangeable parts, easily mount- dismount towards the chassis of the truck  
Side sections (one by each side) for firefighting equipment: 2 pcs  
Adjustable supports for provision parking of the superstructure after the dismount: 4 pcs*

*9.2 Pump:   
Type-membrane: min 40 bar pressure mill. 50 1/minute flow rate  
Gasoline or diesel power generator: min.9 h.p. with an electrical starter;*

*9.3 Reel with installed hose-pipe: min. 50 m, at the rear of the truck;  
Nozzle with spray-module: Included.*

*9.4. STORZ quick connection coupling: Included*

*10. Training of the employers of the Contracting Authority: To 3 working days after the delivery of the supply*

Read: **Firefighting Truck – 1 pc.**

**1. Payload: ≤ 7500 kg**

**2. Movement: at least 4x2**

**3. Engine: Diesel, common rail or similar/or equivalent   
Min. EURO 6  
Min. 115 kW  
Min. 2500 cm3**

**4 Gear box: manual, at least 6+1 gears**

**4.1. optional: Transfer box: Fast and slow gears**

**5 Cabin  
Seats: 2+1  
Air conditioning: Manual  
Driver’s seat: 3-degree adjustable**

**6 Chassis and suspension:   
Semi-elliptical" leaf springs: yes  
Rear turn signal: yes**

**7 Tires: Double rear tires R16, steel wheels 16"**

**8 Water tank:   
Capacity of the water tank: Min. 2000 1**

**9 Special equipment:   
9.1 Fire superstructure with dismount-capacity: easily mount- dismount towards the chassis of the truck  
Side sections (one by each side) for firefighting equipment: 2 pcs  
Adjustable supports for provision parking of the superstructure after the dismount: 4 pcs**

**9.2 Pump:   
Type-membrane: min 40 bar pressure min. 50 1/minute flow rate  
Gasoline or diesel power generator: min. 9 h.p. with an electrical starter;**

**9.3 Reel with installed hose-pipe: min. 50 m, at the rear of the truck;  
Nozzle with spray-module: Included.**

**9.4. STORZ quick connection coupling: Included**

**10. Training of the employers of the Contracting Authority: To 3 working days after the delivery of the supply**

All other terms and conditions of the contract notice remain unchanged. The above alterations and/or corrections to the contract notice are integral part of the contract notice.