**CORRIGENDUM no 1**

**TENDER DOSSIER**

**II.1.1) Contract Notice Title:** Supply of equipment: Tipper truck, Backhoe loader, Skid steer loader, Tractor with trailer

**II.1.1) Contract Notice Reference Number:** CB007.2.31.169 – TD/05

**VII. 1.1) Reason for change**

Modification of original information submitted by the contracting authority.

**VII.1.2) Text to be corrected in the original notice**

**The following alternations and/or corrections are made:**

1. **Section No 16 - Selection criteria in the document Additional information about the Contract Notice - 1) Economic and financial capacity**

Instead of:

* that the tenderer, in the last six months preceding the month in which the Call for Proposals was published, was not illiquid

Proof : the tenderer has to present “Izveštaj o bonitetu” for public procurements (Form БОН-ЈН) issued by the Serbian Business Registers Agency, which has to comprise the following:

* status of the tenderer
* concise balance sheets and profit&loss account for the last 3 years (2018, 2019 and 2020).
* If the prudential Report does not contain information on the days of liquidity in the last six months preceding the month in which the Call for Proposals was published on the Portal, the Tenderer shall submit the Certificate of the National Bank of Serbia that the tenderer in the last six months preceding the month in which the Call for Proposals was published on the Public Procurement Portal, it was not illiquid.

Read:

* that the tenderer, in the last six months preceding the month in which the Call for Proposals was published, was not illiquid

Proof : the tenderer has to present “Izveštaj o bonitetu” for public procurements (Form БОН-ЈН) issued by the Serbian Business Registers Agency, **or equivalent document of foreign country where tenderer have headquarters,** which has to comprise the following:

* status of the tenderer
* concise balance sheets and profit&loss account for the last 3 years (2018, 2019 and 2020).
* If the prudential Report does not contain information on the days of liquidity in the last six months preceding the month in which the Call for Proposals was published on the Portal, the Tenderer shall submit the Certificate of the National Bank of Serbia **or equivalent document of foreign country where tenderer have headquarters,** that the tenderer in the last six months preceding the month in which the Public Call was published, it was not illiquid.

1. **ANNEX II + III: TECHNICAL SPECIFICATIONS + TECHNICAL OFFER – LOT 4**

**Description for the trailer is added:**

**Trailer technical features:**

* Trailer with double height sides
* Capacity(t) 4
* Required tractor power (KW) 25
* Max speed (km/h) 25
* Tires 10.0/75-15"10P
* Weight (kg) 1030
* Tipping system on 3 sides
* Braking system pneumatic

Read:

**LOT4: Tractor with trailer**

|  |  |
| --- | --- |
| **1.DRIVE** | 4WD |
| **2.ENGINE** |  |
| Model | 4100 ELT |
| Hp Category | 75 |
| Rated power (KW) | 52 |
| Type | Diesel, four stroke, 4 cylinders |
| Displacement(cc) | 3707 |
| No. of cylinders | 4 |
| Bore/Stroke (mm) | 100/118 |
| Rated engine RPM | 2000 |
| Max Torque (Nm) | 289 |
| Air cleaner | Dry air cleaner with clogging sensor |
| Cooling | Water, under pressure |
| Fuel injection pump/injectors | BOSCH/BOSCH |
| Oil pressure at rated power speed | 3.5-5.2 |
| Compression Ratio | 18:2:1 |
| Cold-start system / Type | YES, on inlet manifold |
| **3.GEAR BOX AND DIFFERENTIAL** |  |
| Type | Sinhroni |
| No. of gears(forward/ reverse) | 12N+12R |
| Maximum speed (km/h) | 31.9 |
| Differential lock | Yes, foot lock |
| **4.CLUTCH** |  |
| Type | Double |
| Friction plate (lining)-drive / PTO | Ceramic / organic |
| Diameter of friction plate(mm)-drive / PTO | 320 |
| **5.PTO** |  |
| Type | Independent / synchronized |
| RPM | 540/540E (750) |
| Number of splines | 6 |
| Max. Power of PTO(HP) | 55 |
| **6.BRAKES** |  |
| Type | Oil discs |
| Number of brake plates | 5 |
| Parking brake | Yes, Independent |
| Trailer Brake | Yes, air type |
| Type of compressor | Piston type |
| **7.STEERING** |  |
| Type | Power steering |
| Turning radius(m) | 4.53 |
| **8.HYDRAULIC** |  |
| Lifting capacity | 2500 |
| Type of pump | Gear type (MITA) |
| Capacity of pump(lpm) | 45 |
| Options (positioning/draft control) | positioning / draft control |
| 3-point linkage | CAT II |
| Hydraulic jacks | 2 DA / 2 SA |
| **9.ELCTRICAL** |  |
| Battery | 12V,110A |
| Alternator | 12V,90Ah |
| Horn | YES |
| 7-terminal Socket | YES |
| Fuse Box | YES |
| Neutral safety switch | YES |
| P.T.O safety switch | YES |
| Clutch safety switch | YES |
| **10.TYRES** |  |
| Front | 11.2x24 |
| Rear | 16.9x30 (429/85R30) |
| **11.DIMENSIONS AND WEIGHT** |  |
| Wheelbase (mm) | 2345 |
| Overall length (mm) | 4160 |
| Overall width (mm) | 1980 |
| Overall height-rops (mm) | 2520 |
| Overall height-cabin (mm) | 2462 |
| Ground clearence (mm) |  |
| Front axle(mm) | 450 |
| Betveen axles(mm)- without cabin / with cabin | 410 |
| Rear axle(mm) | 570 |
| Front track width (mm) | 1525 |
| Rear track width (mm) | 1510 |
| Weight (Unballasted)-without cabin/with cabin | 3025 / 3300 |
| **12.QUANTITIES** |  |
| Fuel tank capacity(I)-without cabin, with cabin | 78 / 100 |
| Capacity of cooling system(l) | 13.5 |
| Oil in engine(l) | 10.75 |
| Oil in transmission (gear box, differential,  hydraulic)-(l) | 40.35 |
| **13. STANDARD EQUIPMENT** |  |
| ROPS | YES |
| Swinging Drawbar | YES |
| Top link | YES |
| BKT tyres | YES |
| Spare parts kit | YES |
| Tool kit | YES |
| Rear view mirrors-left/right | YES |
| Updraft silincer | YES |
| Mobile Charger Point | YES |
| Liftomatic | YES |
| Weights-front/rear | YES |
| **14. OPTIONAL EQUIPMENT** |  |
| **Cabin** |  |
| Cabin-without AC, with heating | YES |
| Cabin-with AC,with heating | YES |
| ***\*Standard equipment of cabin*** |  |
| -Beacon lights | YES |
| -Fog lights | NO |
| -Rear working lights | YES |
| -Rotating light | YES |
| -Hinged Side glass/Rear glass | YES |
| -Co-Passenger seat | NO |
| -Front & Rear wiper | YES, front |
| Liftomatic | YES |
| Canopy | YES |
| Extra weights-front/rear | YES |
| Radial tyre | YES |
| Downdraft silencer | YES |
| **TRAILER TECHNICAL FEATURES** |  |
| **Trailer with double height sides** | **yes** |
| **Capacity(t)** | **4** |
| **Required tractor power (KW)** | **25** |
| **Max speed (km/h)** | **25** |
| **Tires** | **10.0/75-15"10P** |
| **Weight (kg)** | **1030** |
| **Tipping system on 3 sides** | **yes** |
| **Braking system pneumatic** | **yes** |

**VII.2) Other additional information:**

All other terms and conditions of the contract notice, and tender dossier remain unchanged. The above alterations and/or corrections to the contract notice are integral part of the contract notice and tender dossier.