PR7

F excavation= 3.39

F mound = 0.35

F verge road= 0.18

L pos = 2.40

L subsoil = 1.92

F buffer 1 = 0.16

F buffer 2 = 0.00

F canal= 0.00

L concrete = 1.20

Level

Distance

PR8

F excavation=0.26

F mound = 0.15

F verge road= 0.16

L pos = 2.40

L subsoil = 1.36

F buffer 1 = 0.16

F buffer 2 = 0.00

F canal= 0.00

L concrete = 1.20

Level

Distance

PR9

F excavation= 0.00

F mound = 1.15

F verge road= 0.36

L pos = 2.32

L subsoil = 3.90

F buffer 1 = 0.16

F buffer 2 = 0.00

F canal= 0.00

L concrete = 1.20

Level

Distance

PR10

F excavation=0.00

F mound = 1.16

F verge road= 0.39

L pos = 2.20

L subsoil = 4.23

F buffer 1 = 0.16

F buffer 2 = 0.00

F canal= 0.00

L concrete = 1.20

Level

Distance

PR11

F excavation=0.60

F mound = 0.75

F verge road= 0.18

L pos = 2.20

L subsoil = 2.32

F buffer 1 = 0.16

F buffer 2 = 0.00

F canal= 0.00

L concrete = 1.20

Level

Distance

PR12

F excavation=1.77

F mound = 0.23

F verge road= 0.15

L pos = 2.30

L subsoil = 0.98

F buffer 1 = 0.16

F buffer 2 = 0.00

F canal= 0.00

L concrete = 1.20

Level

Distance

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Designer:    Engineering activities and  technical consultancy,  Dragan Peric,  Bulevar Nemanjica no. 27/11, 18000 Nis | Investor: | City Municipality Crveni Krst- City of Nis | | | |
| Mark of technical documents: | IDP | Project:  CONCEPTUAL DESIGN | MARKS OF WORK PROJECT: 2/2 | |
| Chief Designer:  dr Dragan Peric,  Civil engeener,  License number:  315 0982 03 | Stamp: | Object:  Pedestrian pathway in village Miljkovac, City municipality Crveni Krst | | |
| Date: | | Drawing name: | | Scale:  1:100/1000 |
| 03. December, 2015 | | Cross section | | Number of drawing:  39 |