**PROJECT “HETEROTOPIAS”, CO-FINANCED THROUGH INTERREG-IPA PROGRAMME BULGARIA - SERBIA**

|  |  |
| --- | --- |
| **OPEN AIR MUSEUM** | |
| **TECHNICAL SPECIFICATION** | |
|  | **CONCRETE TABLE**  L**80** cm, B**80** cm, H**70** cm,  reinforced fiber concrete  Surface treatment foundation - custom mosaic, white, UV and waterproofing varnish  Surface treatment table top - polished mosaic, white, UV and waterproofing varnish  Playing fields 3x1 – chess, Nine men's morris and “Man, Don't Get Angry” |
|  | **CONCRETE CHAIR**  L**40** cm, B**40** cm, H**40** cm,  reinforced fiber concrete  Surface treatment foundation - custom mosaic, white, UV and waterproofing varnish  Surface treatment table top - polished mosaic, white, UV and waterproofing varnish |
|  | **CONCRETE BICYCLE STAND**  L**100** cm, B**55** cm, H**26** cm,  high strength reinforced fiber concrete and natural mosaic  Surface treatment - custom mosaic, white, UV and waterproofing varnish  built-in metal rings from stainless steel |
|  | **CHILDREN’S SPRINGBOARD**  Square springboard, for installation in terrain  Standard EN1176, safety zone 23 sq. m,  risk of falling – 1 m, Age group – 3+, number of children – 2, opportunity for children with disabilities – yes,  frame - hot-dip galvanized steel,  Slabs – rubber Euroflex with thickness 30 mm;  Trampoline surface – straps reinforced with steel connected to the frame by steel springs – each one of which with L 185 mm and D20 mm |
| SCHEME  See list 5/9 of the graphic part of the investment project for Open Air Museum | **BENCH PLATFORM**  L**390** cm, B**380** cm,  H**48/40** cm  /48cm installation raft on Klotz/  /40cm installation and backrest above the seat /  Supporting grate for the wooden surface - carbon or low alloy steel, closed profile 30x30mm, powder coated, fasteners – galvanized, powder coated  Indoor installation of concrete walls of Klotz  Wooden planks for seat and backrest – D 12cm, H 6cm, lengths - by size of scheme mandatory on-site control measure, Bulgarian spruce, impregnated for 30 years warranty for protection of atmospheric influences, insecticides and fire |
|  | **CHILDREN’S TRIPLE SWING**  Swing – basket, standard swings – 2 pcs. and swings for babies – 2 pcs.  Standard EN 1176, safety zone 66 sq. m., risk of falling – 1.55 m, Age group – 2+, number of children – 9, opportunity for children with disabilities – yes,  Supporting structure – tubular D125 mm, steel – varnished galvanized, bicolor grey grained coverage with light wavy surface for increased scratch resistance  Horizontal beams – unpainted galvanized steel, PVC sliding rings limiting the abrasion of metal parts, with vandal-proof bracket from stainless steel, rotating bearings, chains and fasteners – from stainless steel  Seats by age:   * a whole piece of rotating polyethylene fixed to a frame from stainless steel, equipped with buffers; * shock-absorbing rubber honeycomb; * polyurethane. |

**ARCH. MARIELA ANDREEVSKA**