# *ANNEX II + III:* TECHNICAL SPECIFICATIONS + TECHNICAL OFFER

**Contract title: Supply of sailing boats and equipment p 1 /…**

**Publication reference:** CB007.2.13.076/LAZARUS/Supply – TD 01

**Columns 1-2 should be completed by the contracting authority**

**Columns 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the contractor's technical offer

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the contracting authority shows the required specifications (not to be modified by the tenderer),
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words ‘compliant’ or ‘yes’ are not sufficient)
* Column 4 allows the tenderer to make comments on its proposed supply and to make eventual references to the documentation

The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.

The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offeredspecifications.

| **1.**  **Item number** | **2.**  **Specifications required** | **3.**  **Specifications offered** | **4.**  **Notes, remarks,  ref to documentation** | **5.**  **Evaluation committee’s notes** |
| --- | --- | --- | --- | --- |
| **1** | Sailing boats – 2 pieces  Minimum requirements:  length – 4,60-4,80m;  width – 1.80-2,00m;  crew – up to 7 persons;  weight – 160-180kg;  vertical surface of sail – 13-15sq.m.  Grot – 9,5 – 11,0sq.m.  Staxel – 3.7-3,8 sq.m. |  |  |  |
| **2** | Outboard engine for sailing boats – 2 pieces  Minimum requirements:  type – 2stroke engine, 1 cylinder;  Power – 5h.p  Volume – 100-110cm2  Ignition system – CDI  Tank – min.2,5l;  Fuel consumption – up to 3 l/h |  |  |  |
| **3** | Trailer for sailing boats – 2 pieces  Minimum requirements:  Trailer for boats with length up to 500sm and width up to 220sm and weight up to 540kg.  Soft suspension, equipped with winch for pulling the boat out of the water on the trailer. |  |  |  |
| **4** | Life jackets – 30 pieces  Minimum requirements:  various sizes,  50N Buoyancy |  |  |  |
| **5** | Megaphone – 1 piece    Minimum requirements:  Power: 15W  Space of activity: 200 meters  Frequency: 500-5000HZ |  |  |  |
| **6** | Anemometer – 1 piece  Minimum requirements:  measurement unit, displaying:  speed of wind;  outside temperature |  |  |  |
| **7** | Paddles – 4 pieces  Minimum requirements:  single aluminium paddle  diameter – 35mm;  foldable |  |  |  |
| **8** | Paddles locker – 4 pieces  Minimum requirements:  material – wood;  connects the paddle to the boat |  |  |  |
| **9** | Neoprene clothing – 20 pieces  Minimum requirements:  various sizes;  one piece 3mm suit, outer and inner lining with Nylon, standard zipper with high-resistant slider |  |  |  |