Hexagonal wooden marquee Scale 1:40

**Technical description:**

Hexagonal wooden marquee made out of fir wood, dimensions 2.40x2.60 (height of the marquee is 4m.), with fence on which the benches are leaning on and table in the middle. Marquee roof is made out of processed boards and all construction is being anchored trough poles by concreting into the base.

Ground plan of Hexagonal wooden marquee Scale 1:40

- Wooden fence

- Wooden bench, thickness 5 cm

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| City Municipality Crveni Krst,  City of Nis,  Street 12. Februar 89,  18000 Nis | Investor: | City Municipality Crveni Krst | | | |
| Project: | Conceptual design of the installation picnic furniture, poles with solar panels and video surveillance at the location Miljkovac- Vidrište | | | |
| Chief Designer:  dr Dragan Peric,  Civil engeener,  License number:  311 4620 03 | Stamp: | Designers:  Suzana Ciric, Civil engineer  Ivana Lukic, architect  Marko Dinic,  Civil engineer | Scale:  1:40 | |
| Date:  5. January2015. | | Drawing name: | | Number of drawing:  13 |
| TECHNICAL DETAIL OF URBAN EQUIPMENT - hexagonal wooden marquee | |